FK 7.1-2                                                                                                                                         To
                                                                                                                                                                  „Kontrol  94” Ltd.
                                                                                                                                                                       Gorna Oryahovitsa

TEST REQUEST
ACCORDING TO THE REQUIREMENTS OF THE EN 16510 STANDARD SERIES
№.................../...................20.......
/ Completed by „Kontrol 94” Ltd. /

	
	1. Data for applicant:
	2. Data for manufacturer:

	Name:
	
	

	Address:
	......................................................................................................................................
...................................................................
	......................................................................................................................................
...................................................................

	Phone / fax, Е-mail:
	
	

	Identification №; 
Tax ID (VAT) №
	......................................................................................................................................
	......................................................................................................................................

	Quality system:
	
	

	Contact person, Phone:
	

	3. Appliance/s for testing:
	............................................................................................................................................
............................................................................................................................................
/ type, name /

	4. Type of appliance/s according to Table 1 of EN 16510-1 and/or Table 9 of EN 16510-2-6:

..................................................................................................................................................................................................................................................................................................................................................................................................................

	

	5. The appliance(s) is/are suitable for connection to a common chimney: 
	
	Yes
	
	No

	                                                                                                                                                      / Please note /

	6. Normative testing documents:
	……………………............…….......................................………………............
/ name of standards, BDS EN, EN, ISO, TS /

	7. Additional specific requirements of the applicant:
	.............................................................................................................................................
............................................................................................................................................
/ designation of Regulation(s); requirements for regional norms; other /

	
	Return of the product after testing:
	
	Yes
	
	No

	
	                                                                  / Please note /
Control sample storage: not stored by the laboratory

	8. Appliance/s to be tested by the following fuel:
	.........................................................................................................................................
/ beech wood logs, coal (briquettes) or both, pellets and etc. /

	8.1. The test fuel is provided by:

	
	
	„Kontrol 94” Ltd.
	
	Applicant

	
	
	
	Certificate of analysis: ..............................


                              / Check your choice /

	9. Reporting of conformity according BDS EN ISO/IEC 17025:2018 and product standards:

	Please report the declaration of conformity according to:

	Note the applicable document - standard
or other regulatory document and at what heat output
	Characteristics
	Requirements

	
	
	Open fronted solid fuel local space heaters
	Closed fronted solid fuel local space heaters using solid fuel other than compressed wood in the form of pellets
	Closed fronted solid fuel local space heaters using compressed wood in the form of pellets

	1
	2
	3
	4
	5
	6

	
	
	EN 16510-2-1:2022

	At nominal heat output:
	At part load head output:
	Carbon monoxide emission (СО) 
at 13%О2
	< 2000 mg/m3
	< 1500 mg/m3
	< 300 mg/m3

	
	
	Nitrogen oxides emissions (NОx) 
at 13%О2
	Appliances, using biomass
	Appliances, using fossil solid fuel

	
	
	
	
	
	
	
	< 200 mg/m3
	< 300 mg/m3

	
	
	Emissions of organic gaseous compounds  (ОGC) at 13%О2
	< 120 mg/m3
	< 120 mg/m3
	< 60 mg/m3

	
	
	Particulate matter emissions (РМ) 
at 13%О2
	< 50 mg/m3
	< 40 mg/m3
	< 20 mg/m3



	1
	2
	3
	4
	5
	6

	
	
	Seasonal space heating efficiency - ηS
	≥ 30 %
	≥ 65 %
	≥ 79 %

	
	
	Temperatures of nearby flammable objects at nominal heat output and temperature safety
	< 65К (65+ Ta)

	
	
	EN 16510-2-2:2022

	At nominal heat output:
	At part load head output:
	Carbon monoxide emission (СО) 
at 13%О2
	< 2000 mg/m3
	< 1500 mg/m3
	< 300 mg/m3

	
	
	Nitrogen oxides emissions (NОx) 
at 13%О2
	Appliances, using biomass
	Appliances, using fossil solid fuel

	
	
	
	< 200 mg/m3
	< 300 mg/m3

	
	
	
	
	
	
	Emissions of organic gaseous compounds  (ОGC) at 13%О2
	< 120 mg/m3
	< 120 mg/m3
	< 60 mg/m3

	
	
	Particulate matter emissions (РМ) 
at 13%О2
	< 50 mg/m3
	< 40 mg/m3
	< 20 mg/m3

	
	
	Seasonal space heating efficiency - ηS
	≥ 30 %
	≥ 65 %
	≥ 79 %

	
	
	Temperatures of nearby flammable objects at nominal heat output and temperature safety
	< 65К (65+ Ta)

	
	
	EN 16510-2-3:2022

	At nominal heat output:
	At part load head output:
	Carbon monoxide emission (СО) 
at 13%О2
	< 2000 mg/m3
	< 1500 mg/m3
	< 300 mg/m3

	
	
	Nitrogen oxides emissions (NОx) 
at 13%О2
	Appliances, using biomass
	Appliances, using fossil solid fuel

	
	
	
	< 200 mg/m3
	< 300 mg/m3

	
	
	
	
	
	
	Emissions of organic gaseous compounds  (ОGC) at 13%О2
	< 120 mg/m3
	< 120 mg/m3
	< 60 mg/m3

	
	
	Particulate matter emissions (РМ) 
at 13%О2
	< 50 mg/m3
	< 40 mg/m3
	< 20 mg/m3

	
	
	Seasonal space heating efficiency - ηS
	≥ 30 %
	≥ 65 %
	≥ 79 %

	
	
	Temperatures of nearby flammable objects at nominal heat output and temperature safety
	< 65К (65+ Ta)

	
	
	EN 16510-2-6:2022

	At nominal heat output:
	At part load head output:
	Carbon monoxide emission (СО) 
at 13%О2
	-
	-
	< 300 mg/m3

	
	
	Nitrogen oxides emissions (NОx) 
at 13%О2
	Appliances, using biomass
	Appliances, using fossil solid fuel

	
	
	
	< 200 mg/m3
	-

	
	
	
	
	
	
	Emissions of organic gaseous compounds  (ОGC) at 13%О2
	-
	-
	< 60 mg/m3

	
	
	Particulate matter emissions (РМ) 
at 13%О2
	-
	-
	< 20 mg/m3

	
	
	Seasonal space heating efficiency - ηS
	-
	-
	≥ 79 %

	
	
	Temperatures of nearby flammable objects at nominal heat output and temperature safety
	< 65К (65+ Ta)

	
	
	EN 16510-2-10:2025

	
	
	Temperatures of nearby flammable objects (at the floor) at temperature safety
	< 65К (65+Ta)

	
	
	Temperatures of nearby flammable objects (without the floor) at temperature safety
	< 65К (65+Ta)

	
	
	Other regulatory document: .......................................................................................

	At nominal heat output:
	At part load head output:
	
	

	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	



Attention:
   When declaring compliance / non-compliance, the laboratory uses a "simple" decision rule according to which there is compliance when the measured value together with the declared uncertainty is within the tolerance range.
   The reported expanded measurement uncertainty had obtained as a work of the standard uncertainty and the coverage multiplier k = 2, which at normal distribution corresponds to a coverage probability of approximately 95%.
   The default probability of conformity is usually (1 - α) = 0,95 (95%) - error type I α = 0,05 (5%), ie the probability that the measured value is within the specified standard must be higher than 95%.
   With a decision-making rule based on simple acceptance and the existence of a normal distribution for the measured value, the probability of accepting a non-compliant element or rejecting a corresponding element may be up to 50%. The risk is then considered a "shared risk" between the laboratory and the client.

	The conformity assessment for the CE marking and Declaration of performance shall be indicated in accordance with the requirements of the product standard and Regulation (EU) 305/2011.

	10. The test report should be issued in:
	
	
	Bulgarian
	
	English


                              / Check your choice /

	11. The laboratory shall: be responsible for all information obtained or created during the test and to inform the applicant in advance if it intends to do properly in public, except in the case where this information is required by authorized and control bodies. 
   The laboratory is responsible for the impartiality of its laboratory activities and does not allow commercial, financial or other pressures to call into question its impartiality.

	12. Additional information:
   The client (applicant) has the right to file a complaint concerning the laboratory activities for which the laboratory is responsible. Upon request, the procedure PK 7.9 "Complaints" is provided to all interested parties. It is available on the laboratory's website as well as the complaint form (FK 7.9-2).
   The laboratory has a hand in the scope of accreditation within the limits described in the Accreditation Certificate and the order to it, as well as in SpK 7.2-3-1, publicly available on the laboratory website.
   The request falls within the flexible scope.
   Laboratory personnel do not report opinions and interpretations, neither in the test reports nor in direct dialogue with the client.

	13. Attachments:
	- The design documentation.
- Instructions for installation and operating.
- Certificates and declarations of conformity for used materials.
- Completed and signed forms for preparation of a test request.
- Marking.
- Declaration of performance.
- Risk assessment (where is applicable).
- Declaration of conformity for LVD – 2014/35/EU; EMC – 2014/30/EU and machinery – 2006/42/ЕС (where is applicable)..

	    I agree to use my personal data in the Laboratory in order to perform laboratory activities of the requested product (s) and issue a test report of the same (s).
   By signing, I certify that I am familiar with and accept the general terms and conditions of the laboratory and undertake to comply with them.

	Data: ……………...
	Applicant:.....................................
/ ..................................... /                                                                                                                                                
/ signature, names and stamp /







Data to be filled in by „Kontrol 94” Ltd.:

[bookmark: _GoBack]I. Declaration of Impartiality: The undersigned’s declare that we have no relationships based on ownership, leadership, management, personnel, shared resources, finances, contracts, marketing (incl. Brands) and payment of commissions from sales or more  to attract customers in relation to the object (s) requested for testing. We know that for incorrect information, liability under Art. 313 of the Penal Code:
	1. ..................... / ................................ /
         / signature /, / analyzer family name /
	2. ..................... / ................................ /
/ signature /, / analyzer family name /
	3. ..................... / ................................ /
/ signature /, / analyzer family name /











II. Risk analysis of impartiality:
	No
	Personnel assigned to perform
the specified test 
	Threats to impartiality,
according to PK 4.1 and FK 4.1-2
(answer the questionnaire after the table with Yes or No)*
	Availability /
Absence
of conflict of interest
(Yes / No)

	
	
	1.1
	1.2
	2.1
	2.2
	3.1
	3.2
	4.1
	4.2
	4.3
	

	1
	
	
	
	
	
	
	
	
	
	
	

	2
	
	
	
	
	
	
	
	
	
	
	

	3
	
	
	
	
	
	
	
	
	
	
	



Questionnaire: In connection with ensuring impartiality and independence of persons designated to carry out the tests of objects in the execution of orders and contracts from customers, the head of the lab asks the following questions to analyze the risk of impartiality and independence of the laboratory.


Threats to impartiality from:
1. Leadership / Management
1.1 Are you in any way connected with the company assigning activities for the implementation of this request?
 (Yes / No)
1.2 Are you a member of the management board of the company assigning activities for the implementation of this request? (Yes / No)
2. Shared resources - personnel, equipment
2.1 Do you work in an employment or other relationship within the company contracting activities in implementing this request? (Yes / No)
2.2 Are you aware of the joint use and /or rental of equipment and premises with the contracting authority in this request?  (Yes / No)
3. Contracts - payment of commissions or other incentives to attract customers
3.1 Do you receive commissions or other incentives from the contracting company for this application in purpose to compromise test results? (Yes / No)
3.2 Have you offered preferences in order to attract the contracting company of this application for our client? (Yes / No)
4.   Personnel
4.1 Have you been involved in the design, manufacture, supply, installation, repair and maintenance of the appliances covered 
by this application? (Yes / No)
4.2 Do you maintain personal relationships (family, friendly or conflicts that have arisen in the past) with personnel members 
of the company assigning this application? (Yes / No)
4.3   Have you participated in any refresher courses organized by the contracting company or have you provided services related to the training of employees of the contracting company in this application? (Yes / No)
* - The risk of impartiality is assessed as follows:
Answer "No" - there is no risk of impartiality, answer "Yes" - there is a threat to impartiality.
In the presence of a risk of impartiality, i.e. answer "Yes" to one of the questions, the Head of the laboratory removes the appointed employee from performing the respective test and evaluates a new one, writing this in a note at the end of the application. 


	Date: ……………...
	Head of laboratory: .........................................
/ eng. Miroslav Raev /



Records of changes in the service of the application after admission to the Laboratory:

..............................................................................................................................................................…………………………….

Notes: ……...............................................……………………………………………………………………………..............…...
..............................................................................................................................................................…………………………….
............................................................................................................................................................………………………..…….
                                         (records of discussions with the client, significant changes, etc.)


	Date: ……………...
	Head of laboratory: .........................................
/ ................................... /
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